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                                      Technology Paper


                         6090 DSP 
There are 2 parts here.  一. Inner Format .  二 . Parameters on the DSP

1.  Inner Format . 

Step: MENU--SYSTEM  SETUP--Inner Format 
二 . Parameters on the DSP 
1. MENU--MACHINE SETUP--Pulse Equiv:  X  Axis： 320 
                                    Y  Axis： 320 
                                    Z  Axis：160 
2. MENU--MACHINE SETUP--Table Size:  X  Axis：610
                                  Y  Axis：910 
                                  Z  Axis： 150 
3.MENU--MACHINE SETUP--Home Setup--Home Direction:   X  Axis：-Dir
                                                 Y  Axis：-Dir
                                                 Z  Axis：+Dir

4. MENU--MACHINE SETUP--Spindle Setup

Step1. Input Spindle st :8

Step2.Press button OK

Step3. Line State when spindle is off :   0  1  2  3  

                             ↓  ↓  ↓  ↓

Step4. Press button OK

Step5. Line state of 1s grade speed:   0  1  2  3

                            ↑   ↓  ↓  ↓

Step6 . Press button OK

  Step7. Line state of 2s grade speed:    0  1  2  3

                             ↓  ↑  ↓  ↓

Step8. Press button OK

  Step9. Line state of 3s grade speed:   0  1  2  3

                             ↑  ↑  ↓  ↓

Step10. Press button OK

  Step11. Line state of 4s grade speed:   0  1  2  3

                             ↓  ↓  ↑  ↓

Step12. Press button OK

  Step13. Line state of 5s grade speed:   0  1  2  3

                             ↑  ↓  ↑  ↓

Step14. Press button OK

  Step15. Line state of 6s grade speed :  0  1  2  3

                             ↓  ↑  ↑  ↓

Step16. Press button OK

Step17. Line state of 7s grade speed:   0  1  2  3

                             ↑  ↑  ↑  ↓

Step18. Press button OK

5.  Voltage Setup：

Input Volt:
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Output Volt: no need to change
6. MENU--MACHINE SETUP--C.A.D thickness: 10

7. MENU--AUTO PRO SETUP--Linear Accl:  600 
8. MENU--AUTO PRO SETUP--Curv Accl:  800 
9.  Speed of the machine: 
There are 2 kinds of speed, high speed and low speed. Both of the 2 speed are needed to set. On the interface next, press high/low to change each other. 
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A. Press "CANCEL", you can find the speed 

B. press “DELETE" you can change the figure of the speed, here you can use button "X+/X-"to cut to X axis, Y axis, Z axis.  Each time you input the figures do not forget to press "OK".

 Followed are the figures of your machine.
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The High Speed may change to be X 8000, Y 8000, Z 2000 for RJ6090 . 
