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Fin | signal Comment
1 |PULSE+ | PULSE, to drive side
2 |DIR+ DIRECTION, to drive side
3 |ENAT ENABLE, fo diive side
4 | BERO Zero mark, from drive side
m 5 [~2av POWER from the pin 1 of X200, +24V output
6 |RST ALARM RESET, to drive side
7 |24 Ground
3 5 24V POWER from the pin 1 of X200, +24V output
9 [PULSE- | NEGATIVE PULSE, fo drive side
10 [ DIR- NEGATIVE DIRECTION, to drive side.
11 ENA- NEGATIVE ENABLE, to drive side
12 [+2av POWER from the pin 1 of X200, +24V output
13 | M24 Ground
14 | RDY, DRIVE READY, from drive side
15 | ALM ALARM, from drive side
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SERVOPACK SGDV-5R4D01A + SERVOMOTOR SGMGV-13DDA6F
	Pin CN1
	Function

	40   /S-ON
	Servo ON/OFF: Turns ON/OFF the servomotor.

	41 /P-CON
	

	42   P-OT
	

	43    N-OT
	

	44  /ALMRST
	Alarm reset: Releases the servo alarm state.

	47  +24VIN
	

	5(6)  V-REF
	Inputs speed reference. Input voltage range: 12 V max.

	7      PULS
	Input pulse modes: Set one of them.

- Sign + pulse string

- CCW/CW pulse

- Two-phase pulse (90 phase differential)

	8      / PULS
	

	11     SIGN
	

	12     /SIGN
	

	15       CLR
	Position error pulse clear: Clears position error pulse during position control.

	14      /CLR  
	

	FG
	Ground

	31    ALM+
	Servo alarm: Turns OFF when an error is detected.

	32    ALM-
	

	27   /TGON+ 
	Detection during servomotor rotation: Turns ON when the servomotor is rotating at a speed higher than the motor speed setting.

	28   /TGON-
	

	29   /S-RDY+
	Servo ready: ON when the SERVOPACK is ready to accept the servo ON (/S_ON) signal.

	30   /S-RDY-
	

	33    PAO
	

	34    /PAO
	

	35    PBO
	

	36    /PBO
	

	19    PCO
	

	20    /PCO
	

	25   /V-CMP+
	Turns ON when whether the motor speed is within the setting range is detected and if it matches the reference speed value.

	26   /V-CMP-
	

	3         PL1
	Output signals of power supply for open-collector reference

	13        PL2
	

	18       PL3
	

	25    /COIN+
	Turns ON when the number of position error pulse reaches the value set.

	26    /COIN-
	


ЧПУ


                                                                                                                                     ???
                                       
                                                                                                                        ???
Как соединить ЧПУ «SINUMERIK 808D» с цифровым управлением приводами с приводом SERVOPACK SGDV-5R4D01A?

Стрелками обозначены мои предположения (они могут быть не верными).
